**WEEKLY PROBE THERMOMETER CONDITION/ PERFORMANCE CHECK LOG**

**FORM 18**

**Hotel:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Probe**  **Number** | **Date** | **Temp’ Achieved**  **On Test** | | **Condition and Corrective Action Taken** | **Signature** |
| **Boiling water** | **Iced water** |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

**Tolerances Corrective Action**

|  |  |  |  |
| --- | --- | --- | --- |
| **Iced water** | Stir the probe in a mixture of ice and a small amount of water until a steady reading is achieved. This should read between -1ºC to +1ºC. |  | * If outside this range, the unit should be returned to the manufacturer or discarded. |
| **Boiling water** | Agitate the probe in boiling unsalted water until a steady reading is achieved. This should read between 99ºC and 101ºC. |  |